Taylor Earl

11/23

* Remove login
  + Who interprets the characters (login)
* TELNET
  + Transform key presses into the NVT (Network virtual terminal)
  + o - normal
  + i - control
  + all 1’s = IAC =
  + Options
    - Binary
    - Echo
    - Surpress Go-ahead
    - Terminal Type
    - Speed
  + Negotiation
    - WILL
    - WON’T
    - DO
    - DON’T
  + Other Control characters
    - IP
      * Interupt Process
    - AO
      * Abort Output
    - AYT
      * Are you there
    - EC
      * Erase Character
* Telnet
  + Uses TCP - 23
* SSH
  + TCP - 22
    - Establish a connection
    - Authenticate the server
      * Secure Channel
    - Authenticate the client
      * Multiplexing source
* FTP
  + File Transfer Protocol
  + TCP - 21, 20